{"text_format":"3","workbook":"xls","n_sheets":13,"sheets":["公司本部","大羊坊","廊坊","采育","机场站","杨村所","军粮城所","马驹桥所","罩棚维修","泗村店","总价措施费","总费用表","单价构成分析表"],"not_rendered":{"images":7,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"公司本部","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（本部）"]
["子目号","子目名称","单位","数量","单价","合价"]
["GS-001-001","原有屋面旧防水清除、清扫、废料外运，破损处M7.5防水砂浆找平，刷冷底子2遍，油粘铺2层3厚单面自贴型玻纤胎SBS改性沥青防水卷材","m2",570,null,{"v":0,"d":"0.00"}]
["GS-001-005","院区地面石材更换(原有石材挖除，废料外运，填砂压实，更换石材，材质花岗岩如原有材较好，可重复利用)","m2",350,null,{"v":0,"d":"0.00"}]
{"$rows_empty":13}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"大羊坊","index":1,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（大羊坊）"]
["子目号","子目名称","单位","数量","单价","合价"]
["DYF-002-001","屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材","m2",450,null,{"v":0,"d":"0.00"}]
{"$rows_empty":18}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"廊坊","index":2,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（廊坊）"]
["子目号","子目名称","单位","数量","单价","合价"]
["LF-004-001","屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材（主楼800m2，食堂400m2，电工房、浴室300m2）","m2",1500,null,{"v":0,"d":"0.00"}]
["LF-004-002","更换木门（（拆除原有木门，门框，垃极运输、安装新门框及木门, (单开门0.9*2，29扇、双开门1.4*1.9，1扇，颜色与原有同）","扇",30,null,{"v":0,"d":"0.00"}]
["LF-004-003","断桥铝门窗（拆除原铝合金门窗、垃圾清运、安装断了的断桥铝门窗（55型，双玻）","m2",20,null,{"v":0,"d":"0.00"}]
["LF-004-004","二层木门维修","扇",5,null,{"v":0,"d":"0.00"}]
{"$rows_empty":15}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"采育","index":3,"n_rows":23,"n_cols":8,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（采育）"]
["子目号","子目名称","单位","数量","单价","合价"]
["CY-003-001","厕所维修"]
["CY-003-001-01","蹲便器（拆除、得新安装）","个",12,null,{"v":0,"d":"0.00"}]
["CY-003-001-02","脚踏冲洗阀（拆除，重新安装）","个",12,null,{"v":0,"d":"0.00"}]
["CY-003-001-03","小便器（拆除原建筑，安装新器具）","个",6,null,{"v":0,"d":"0.00"}]
["CY-003-001-04","隔位门（拆除原有，安装新隔位门）","套",12,null,{"v":0,"d":"0.00"}]
["CY-003-001-05","地面维修(拆除原地面、重新防水、砼找平层、砌筑新的磁砖地面，300*300)","m2",100,null,{"v":0,"d":"0.00"}]
["CY-003-001-06","上水管更新（DN60分，PPR管挖开地面、拆除原管、更换上水管）","m",50,null,{"v":0,"d":"0.00"}]
["CY-003-001-07","下水管更新（DN75，PPR管，挖开地面、拆除原管、更换上水管）","m",60,null,{"v":0,"d":"0.00"}]
["CY-003-002","门窗更换",{"$nulls":3},{"v":0,"d":"0.00"}]
["CY-003-002-001","木门更换（拆除原有木门，门框，垃极运输、安装新门框及木门， (单扇0.9*2，33个、双扇1.4*2，1扇，颜色与原有同）","扇",34,null,{"v":0,"d":"0.00"}]
["CY-003-002-002","办公楼大门双开玻防璃门更换（包括地璜、双开玻璃门、门禁,(双开门,3*3.3)）","套",1,null,{"v":0,"d":"0.00"}]
["CY-003-002-003","吊顶更换（吊顶与原有材质、规格相同）","m2",30,null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":7}," "]
[]
[]
[]
[]
[]
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"机场站","index":4,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（机场）"]
["子目号","子目名称","单位","数量","单价","合价"]
["JC-005-001","屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材","m2",1000,null,{"v":0,"d":"0.00"}]
["JC-005-002","二楼男、女卫生间小洗浴室防水维修（地面拆除、防水新做、安装地漏，找平、安装地砖）","m2",20,null,{"v":0,"d":"0.00"}]
{"$rows_empty":17}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"杨村所","index":5,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（杨村所）"]
["子目号","子目名称","单位","数量","单价","合价"]
["YC-008-001","屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材","m2",1300,null,{"v":0,"d":"0.00"}]
["YC-008-002","吊顶更换（拆除破损的吊顶、清运垃圾、更换新吊顶，吊顶采用材质与原有吊棚相同）","m2",130,null,{"v":0,"d":"0.00"}]
["YC-008-003","更换地砖（拆除原有地砖、清运垃圾、M10水泥砂浆找平层、铺砌新地砖，地砖与原有材质、规格相同）","m2",50,null,{"v":0,"d":"0.00"}]
["YC-008-004","重新包门窗垭口","m2",20,null,{"v":0,"d":"0.00"}]
{"$rows_empty":15}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"军粮城所","index":6,"n_rows":19,"n_cols":6,"rows_kept":19,"merged":[[0,0,0,5],[13,0,13,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（军粮城所）"]
["子目号","子目名称","单位","数量","单价","合价"]
["JLC-009-001","屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材","m2",660,null,{"v":0,"d":"0.00"}]
["JLC-009-002","男女浴室淋浴设施更换，拆除原有淋浴设施、清运垃圾、更新淋浴花洒，全铜花洒套装，不锈钢增压顶喷","套",6,null,{"v":0,"d":"0.00"}]
["JLC-009-003","男女浴室更换地砖，拆除原有地砖、清运垃圾、M10水泥砂浆找平层、铺砌新地砖。墙砖挑选须与使用单位工作人员共同挑选","m2",40,null,{"v":0,"d":"0.00"}]
["JLC-009-004","男女浴室吊顶更换，拆除原有吊顶，清运垃圾，铝扣板吊顶，吊顶挑选须与使用单位人员共同挑选","m2",40,null,{"v":0,"d":"0.00"}]
["JLC-009-005","男女浴室更换地砖，拆除原有墙砖、清运垃圾、M10水泥砂浆找平层、铺砌新墙砖。墙砖颜色质量需与使用单位的人共同挑选","m2",130,null,{"v":0,"d":"0.00"}]
["JLC-009-004","男女浴室排水管道（室内、室外）更换，拆除原有淋浴设施、清运垃圾、",{"$nulls":3},{"v":0,"d":"0.00"}]
["JLC-009-004-001","男女浴室100mmPPR热容管更换（更换室内排水管，更换地漏5个，不锈钢地漏）","m",40,null,{"v":0,"d":"0.00"}]
["JLC-009-004-002","男女浴室外D200mm水泥排水管更换（挖除地面及填土，夯实基底，5cm碎石垫层，更换水泥管，回填土至地面，恢复地面）","m",40,null,{"v":0,"d":"0.00"}]
["JLC-009-005","大厅、楼道、会议室屋顶内墙维修(铲除原有内墙，清理干净，原墙面为砼，则聚合物砂浆找平补腻子、打磨、重新粉刷乳胶漆","m2",800,null,{"v":0,"d":"0.00"}]
[]
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null," "]

{"sheet":"马驹桥所","index":7,"n_rows":30,"n_cols":6,"rows_kept":30,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（马驹桥所）"]
["子目号","子目名称","单位","数量","单价","合价"]
["MJQ-007-001","顶棚铝扣板吊顶维修","m2",300,null,{"v":0,"d":"0.00"}]
["MJQ-007-002","屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材（马驹桥西站650m2，马驹桥所300m2）","m2",950,null,{"v":0,"d":"0.00"}]
{"$rows_empty":17}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[]
[]
[{"$nulls":3}," "]

{"sheet":"罩棚维修","index":8,"n_rows":39,"n_cols":6,"rows_kept":39,"merged":[[0,0,0,5],[38,0,38,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（罩棚维修）"]
["子目号","子目名称","单位","数量","单价","合价"]
["ZP-010-001","泗村店罩棚维修(杆件更换、排水管更新、站区字牌除锈、维修)8个车道，罩棚长约60米宽25米，罩棚上面层遮阳板有损坏脱落，需维修或更换。5吋排水管总数16棵，每棵约12米，目测约100米损坏。站区字牌8个字，约30平米。罩棚侧面外围约85平米需维修油饰。罩棚内部杆件数量较多，需维修或油饰。",{"$nulls":3},{"v":0,"d":"0.00"}]
["ZP-010-001-001","罩棚钢杆件除锈，刷防锈漆二遍，刷色漆一遍，颜色与原色同，蓝灰色","m2",1500,null,{"v":0,"d":"0.00"}]
["ZP-010-001-002","更换遮阳板(清除原有遮阳板，清运垃圾，更新新板10mm，4层蜂窝状，1.7Kg，打胶钉铝条，支撑遮阳板的20mm镀锌不锈钢方管如损坏进行更换)","m2",550,null,{"v":0,"d":"0.00"}]
["ZP-010-001-003","排水管更换（排水管d=5寸，管材与原有材质同，镀锌不锈钢管）","m",192,null,{"v":0,"d":"0.00"}]
["ZP-010-001-004","站区字牌油饰(除掉原有色漆或锈，刷二遍防锈漆，刷色漆，颜色与原色同）","m2",30,null,{"v":0,"d":"0.00"}]
["ZP-010-001-005","罩棚侧面油饰（除掉原有色漆或锈，刷二遍防锈漆，再刷一遍色漆，颜色与原漆色相同）","m2",85,null,{"v":0,"d":"0.00"}]
["ZP-010-002","空港站罩棚硅酮密封耐候打胶（，罩棚铝板接缝处密封胶老化漏雨，新打胶并维修加固，剔除旧胶，新胶采用硅酮耐候密封胶，可以用于玻璃与铝板的粘贴、铝板与铝板之间的粘贴，铝板厚4mm，缝宽15mm）","m2",90,null,{"v":0,"d":"0.00"}]
["Zp-010-003","空港站罩棚屋面防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材","m2",1950,null,{"v":0,"d":"0.00"}]
["ZP-010-004","杨村站罩棚维修（遮阳板、杆件除锈、排水管维修、华北蓝外延维修）（罩棚面积约长65米宽20米高3米，内部杆件较多需维修油饰。遮阳板约40平米。排水管120米。站区字牌金字10个，约35平米，蓝字10个，约10平米）",{"$nulls":3},{"v":0,"d":"0.00"}]
["ZP-010-004-001","遮阳板更换(原有遮阳板拆除，垃圾清运、更换新的遮阳板，更新新板10mm，4层蜂窝状，1.7Kg，打胶钉铝条，支撑遮阳板的20mm镀锌不锈钢方管如损坏进行更换)","m2",40,null,{"v":0,"d":"0.00"}]
["ZP-010-004-002","站区字牌金字油饰(除锈，除原有色漆，重校报刷防锈漆，漆色与原来同，10个字)","m2",35,null,{"v":0,"d":"0.00"}]
["ZP-010-004-003","站区字牌蓝字油饰(除绣，除原有色漆，重新刷防锈漆，漆色与原来同，10个字)","m2",10,null,{"v":0,"d":"0.00"}]
["ZP-010-004-004","华北蓝装饰维修（彩钢板骨架除锈，刷防锈漆二遍）","m2",510,null,{"v":0,"d":"0.00"}]
["ZP-010-004-005","华北蓝装饰维修（彩钢板饰面）","m2",510,null,{"v":0,"d":"0.00"}]
["ZP-010-004-006","华北蓝装饰维修（彩钢板拉撑钢架除锈，刷防锈漆二遍）","m",255,null,{"v":0,"d":"0.00"}]
["ZP-010-004-007","罩栅钢构除锈除漆 刷防锈漆二遍","m2",1300,null,{"v":0,"d":"0.00"}]
["ZP-010-005","塘沽站罩棚维修(华北蓝外延维修，罩棚约长80米宽25米高2米，8个排水口漏水)",{"$nulls":3},{"v":0,"d":"0.00"}]
["ZP-010-005-001","华北蓝装饰维修（彩钢板骨架除锈，刷防锈漆二遍）","m2",318.4,null,{"v":0,"d":"0.00"}]
["ZP-010-005-002","华北蓝装饰维修（彩钢板拉撑钢架除锈，刷防锈漆二遍）","m",162,null,{"v":0,"d":"0.00"}]
["ZP-010-005-003","华北蓝装饰维修（彩钢板饰面）","m2",318.4,null,{"v":0,"d":"0.00"}]
["ZP-010-006-001","塘沽西站主站构架、罩棚维修(罩棚约长50米宽25米，罩棚有漏雨现象，原铝扣板脱落。最边一跨约长35米)",{"$nulls":3},{"v":0,"d":"0.00"}]
["ZP-010-006-002","原有铝塑板及钢骨架拆除","m2",523.53,null,{"v":0,"d":"0.00"}]
["ZP-010-006-003","钢骨架焊接及安装部分","m2",523.53,null,{"v":0,"d":"0.00"}]
["ZP-010-006-004","铝塑板加工及安装","m2",523.53,null,{"v":0,"d":"0.00"}]
["ZP-010-006-005","收费厅侧面重新安装钢骨架","m2",88.08,null,{"v":0,"d":"0.00"}]
["ZP-010-006-006","铝扣板顶安装轻钢龙骨","m2",523.53,null,{"v":0,"d":"0.00"}]
["ZP-010-006-007","铝扣板顶加装吊杆","m2",523.53,null,{"v":0,"d":"0.00"}]
["ZP-010-006-008","重新制作排水槽","m",30,null,{"v":0,"d":"0.00"}]
["ZP-010-006-009","雨蓬灯（菲利浦LED，60W）","套",32,null,{"v":0,"d":"0.00"}]
["ZP-010-006-010","密封结构胶及敷料（硅酮耐候胶）","m2",523.53,null,{"v":0,"d":"0.00"}]
["ZP-010-007","塘沽西分站构架、罩棚维修(罩棚约长40米宽15米。罩棚有漏雨现象，顶板约三分之一破损)",{"$nulls":3},{"v":0,"d":"0.00"}]
["ZP-010-007-001","罩棚防水。原有屋面旧防水清除、清扫、废料外运，破损处DS砂浆找平，再刷一层DFZ-C聚合物水泥基防水涂料，，粘贴3厚自粘型玻纤胎SBS改性沥青防水卷材","m2",600,null,{"v":0,"d":"0.00"}]
["ZP-010-007-002","铝扣板加工及安装(原有铝扣板拆除，清运，杆件除锈刷防锈漆二遍，安装新铝塑板)","m2",200,null,{"v":0,"d":"0.00"}]
["ZP-010-007-003","雨蓬灯（LED，60W）","套",24,null,{"v":0,"d":"0.00"}]
["ZP-010-007-004","密封结构胶及敷料","m2",200,null,{"v":0,"d":"0.00"}]
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"泗村店","index":9,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程（泗村店）"]
["子目号","子目名称","单位","数量","单价","合价"]
["SC-011-001","办公楼外墙维修（破损处墙面铲除，水泥砂浆找平，贴50mm厚A级阻燃板保温，挂金属网，抹砂浆，外刷颜色料防水涂料3遍,檐口防雨处理，深棕色60m2，乳白色80m2）","m2",140,null,{"v":0,"d":"0.00"}]
{"$rows_empty":18}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"总价措施费","index":10,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,5],[22,0,22,1]],"flags":["formulas_cached_only"]}
["工程量清单"]
["工程名称：京津塘高速公路2016年房建维修工程"]
["子目号","子目名称","单位","数量","单价","合价"]
["ZZ-001","按合同条款规定，提供建筑工程一切险（费率3‰）","项",1,null,{"v":0,"d":"0.00"}]
["ZZ-002","按合同条款规定，提供第三者责任险（100万的费率3.5‰）","项",1,null,{"v":0,"d":"0.00"}]
["ZZ-003","安全生产费（整个工程所需安全防护、安全措施费用，费率2.5%）","项",1,null,{"v":0,"d":"0.00"}]
["ZZ-004","竣工文件编制费（编制竣工文件所需费用）","项",1,null,{"v":0,"d":"0.00"}]
{"$rows_empty":15}
["本页小计",{"$nulls":4},{"v":0,"d":"0.00"}]

{"sheet":"总费用表","index":11,"n_rows":15,"n_cols":2,"rows_kept":15,"merged":[[0,0,0,1]],"flags":["formulas_cached_only"]}
["投标报价汇总表"]
["京津塘高速公路2016年专项工程房建维修工程施工"]
["汇总内容","金额（元）"]
["公司本部",{"v":0,"d":"0.00"}]
["大羊坊站",{"v":0,"d":"0.00"}]
["廊坊站",{"v":0,"d":"0.00"}]
["采育站",{"v":0,"d":"0.00"}]
["机场站",{"v":0,"d":"0.00"}]
["杨村所",{"v":0,"d":"0.00"}]
["军粮城所",{"v":0,"d":"0.00"}]
["马驹桥所",{"v":0,"d":"0.00"}]
["罩棚维修",{"v":0,"d":"0.00"}]
["泗村店",{"v":0,"d":"0.00"}]
["总价措施费",{"v":0,"d":"0.00"}]
["清单小计",{"v":0,"d":"0.00"}]

{"sheet":"单价构成分析表","index":12,"n_rows":3,"n_cols":9,"rows_kept":3,"merged":[[0,0,0,8],[1,0,2,0],[3,0,4,0],[5,0,6,0],[7,0,8,0],[9,0,10,0],[11,0,12,0],[13,0,14,0],[15,0,16,0],[17,0,18,0],[19,0,20,0]],"flags":["formulas_cached_only"]}
[" 工程项目单价构成分析表"]
["项\n目\n号","项目说明","工序1","工序2","工序3",null,null,"…","工序N"]
[null,"综合单价  \n(1)+(2)+...(N)","分项单价 \n ( 1 )","分项单价 \n (2 )","分项单价 \n ( 3 )",null,null,"…","分项单价 \n ( N )"]